(module ldtSwitchOBSOLETE:SS_13PLP (layer F.Cu) (tedit 53E93CF1)
  (fp_text reference SS_13PLP (at 0.1 6.2) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value VAL** (at 0.1 4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -7.8 2) (end 7.8 2) (layer F.SilkS) (width 0.15))
  (fp_arc (start 0 13) (end 1.8 13) (angle 90) (layer F.SilkS) (width 0.15))
  (fp_arc (start 0 13) (end 0 14.8) (angle 90) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.8 10.1) (end 1.8 13) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.8 10.1) (end -1.8 13) (layer F.SilkS) (width 0.15))
  (fp_line (start 7.8 10.1) (end 7.8 -1.4) (layer F.SilkS) (width 0.15))
  (fp_line (start -7.8 10.1) (end -7.8 -1.4) (layer F.SilkS) (width 0.15))
  (fp_line (start 7.8 10.1) (end -7.8 10.1) (layer F.SilkS) (width 0.15))
  (fp_line (start -7.8 -1.4) (end 7.8 -1.4) (layer F.SilkS) (width 0.15))
  (pad 2 thru_hole circle (at 0 0) (size 2 2) (drill 1.4) (layers *.Cu *.Mask F.SilkS))
  (pad 1 thru_hole circle (at -4.7 0) (size 2 2) (drill 1.4) (layers *.Cu *.Mask F.SilkS))
  (pad 3 thru_hole circle (at 4.7 0) (size 2 2) (drill 1.4) (layers *.Cu *.Mask F.SilkS))
  (pad 4 thru_hole circle (at 6.605 9.53) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (pad 5 thru_hole circle (at -6.605 9.53) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (model ${HOME}/mnt/KiCadLib/3DModels/Switch/SS_13PLP.wrl
    (at (xyz 0 0 0.001))
    (scale (xyz 0.394 0.394 0.394))
    (rotate (xyz 0 0 0))
  )
)
