(module NR-J6HF (layer F.Cu) (tedit 53E78D07)
  (fp_text reference NR-J6HF (at -5.5 0.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value VAL** (at -5.5 -1.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -24 -9.5) (end 0 -9.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 0 -9.5) (end 0 -6) (layer F.SilkS) (width 0.15))
  (fp_line (start 0 -6) (end 9 -6) (layer F.SilkS) (width 0.15))
  (fp_line (start 9 -6) (end 9 6) (layer F.SilkS) (width 0.15))
  (fp_line (start 9 6) (end 0 6) (layer F.SilkS) (width 0.15))
  (fp_line (start 0 6) (end 0 6.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 0 6.5) (end -24 6.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -24 6.5) (end -24 -9.5) (layer F.SilkS) (width 0.15))
  (pad S thru_hole circle (at -4.25 -7.23) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad R thru_hole circle (at -10.6 -7.23) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad T thru_hole circle (at -16.95 -7.23) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad SN thru_hole circle (at -4.25 4.2) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad RN thru_hole circle (at -10.6 4.2) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad TN thru_hole circle (at -16.95 4.2) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at -13.8 -5.1) (size 3 3) (drill 3) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at -7.45 -7.23) (size 2 2) (drill 2) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at -7.45 4.2) (size 2 2) (drill 2) (layers *.Cu *.Mask F.SilkS))
  (model ${HOME}/mnt/KiCadLib/3DModels/Connector/NR-J6HF.wrl
    (at (xyz 0 0 0))
    (scale (xyz 0.394 0.394 0.394))
    (rotate (xyz 0 0 0))
  )
)
