(module LW_G6CP (layer F.Cu) (tedit 58CD2BCA)
  (descr https://jupiter4.fritz.box/~development/ComponentSheets/Osram/LW_G6CP.pdf)
  (tags "PLCC, PLCC-6")
  (fp_text reference LED** (at 2.794 0 270) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value LW_G6CP (at -2.54 0 90) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 1.778 1.016) (end 1.778 -1.778) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.778 1.778) (end 1.778 1.524) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.778 1.778) (end -1.778 -1.778) (layer F.SilkS) (width 0.15))
  (pad A smd rect (at -1.05 1.7) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad NC smd rect (at 0 1.7) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask))
  (pad A smd rect (at 1.05 1.7) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad A smd rect (at -1.05 -1.7) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad A smd rect (at 1.05 -1.7) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad K smd rect (at 0 -1.7) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask))
  (model /home/thomas/mnt/KiCadLib/3DModels/Diodes/LW_G6CP.wrl
    (at (xyz 0 0 0))
    (scale (xyz 0.3937 0.3937 0.3937))
    (rotate (xyz 0 0 0))
  )
)
