(module NS-J12HL (layer F.Cu) (tedit 53E7A778)
  (fp_text reference NS-J12HL (at -11.5 0) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value VAL** (at -11.5 -2) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -24.5 -10) (end 0 -10) (layer F.SilkS) (width 0.15))
  (fp_line (start 0 -10) (end 0 -6) (layer F.SilkS) (width 0.15))
  (fp_line (start 0 -6) (end 8.5 -6) (layer F.SilkS) (width 0.15))
  (fp_line (start 8.5 -6) (end 8.5 6) (layer F.SilkS) (width 0.15))
  (fp_line (start 8.5 6) (end 0 6) (layer F.SilkS) (width 0.15))
  (fp_line (start 0 6) (end 0 7) (layer F.SilkS) (width 0.15))
  (fp_line (start 0 7) (end -24.5 7) (layer F.SilkS) (width 0.15))
  (fp_line (start -24.5 7) (end -24.5 -10) (layer F.SilkS) (width 0.15))
  (pad G thru_hole circle (at -1.73 -5.96) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad SB thru_hole circle (at -4.61 -7.23) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad ST thru_hole circle (at -7.78 -8.5) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad RB thru_hole circle (at -10.95 -7.23) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad RT thru_hole circle (at -14.13 -8.5) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad TB thru_hole circle (at -17.3 -7.23) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad TT thru_hole circle (at -20.48 -8.5) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad SNB thru_hole circle (at -4.61 5.47) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad SNT thru_hole circle (at -7.78 4.2) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad RNB thru_hole circle (at -10.95 5.47) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad RNT thru_hole circle (at -14.13 4.2) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad TNB thru_hole circle (at -17.3 5.47) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad TNT thru_hole circle (at -20.48 4.2) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (model ${HOME}/mnt/KiCadLib/3DModels/Connector/NS-J12HL.wrl
    (at (xyz 0 0 0))
    (scale (xyz 0.394 0.394 0.394))
    (rotate (xyz 0 0 0))
  )
)
